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Product Details - The Ultra Water Bottle filters use a proprietary patented electro-positive filter media that rapidly adsorbs particles, as small as a few nanometers. 
· Advanced Ultra Filtration
· NSF-42, 53, 61, 372 certified 
· No Chemicals
· Filters Heavy Metals, Lead, Mercury
· Chlorine, Bacteria, Virus, Cysts, Particulate Removal
· 200 Gallon capacity 
· Low cost to maintain
· Easy to maintain
· Great tasting water
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Unit Price:		$599.00
Tax (Varies)		$		
Shipping  (Varies)	$		
Total			$		
Never question what is in your water again.

SKU 50801-01 Shop | Emergency Water Kit
Filtration System for (straws) 350 – (bottle) 500 Gallons

Quality Water While on the Go or Emergency.
The Ultra Water Bottle is your clean water solution for you anywhere you need a refill and can’t trust the source. It creates healthy water for drinking anywhere, anytime. Our filtration system uses the same technology used by NASA. It filters water with no chemicals. Ultra Water Bottle creates healthy and great tasting water for you to enjoy.
Purer Then Bottled Water

Saving the planet, replacing bottled water with UltraHome Filtration System.
· No Chemicals.
· 99.999999% Removal of Bacteria
· >99.99% Removal of Spores, Bacteria, Cysts
· Viruses, pathogens, mold, fungus
· ‘Allowable Toxins’ – chlorine
· Heavy Metals, Micro-Plastics
· Pesticides, Pharmaceuticals
· Adding Micro-Nutrients & Minerals for Optimum Health benefits
· Eco-Friendly
· Eliminates the use for plastic water bottles
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