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Adds minerals and micro-nutrients                                 
Whole-Home Water. Reengineered.  Hyperlinked to Whole Home Video
Designed for Municipal and Well Water Supply
The Facts
•99.9999999% bacteria removal (>9 LRV*)
•99% reduction of heavy metals (97.2% lead reduction)
•95% reduction of PFAS (forever chemicals, PFOA/PFOS)
•Anti-scale filter to treat hard water
•No water softener needed
•No heavy bags of salt
•No salinized wastewater
•Reduces the scale buildup on faucets, cookware, appliances; leave good minerals in water
•Particulate reduction down to 20 nm.

Step 1 - Uses a multi-faceted filter, removing large particles - greater than 5 micron.  Simultaneously conditioning the incoming water so it can no longer form calcium carbonate – no more spots when cleaning, dishes, silverware.  This filtration process extends the life.
MicronGuard™ our next stage, filters out sediment. Conditions water so glasses and faucets remain spotless.

Step 2 - Uses our proprietary MicronGuard™ filter, removing bacteria, viruses, cysts, spores, and other pathogens. Engineered with an activated carbon high surface area paper reduces pathogens, pesticides, pharmaceuticals, forever chemicals (PFOA/PFOS), and heavy metals (including lead). We incorporate Agion silver particles preventing the filter from biofouling.

Step 3 - Stage 3 is the Final polishing of PFOA/PFOS, lead, chlorine, pesticides, and other contaminants with a high-capacity carbon filter. This improves taste and smell of water.  This carbon will outperform similar carbons due to the purity of water at this step of the process.
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Step 1: Proprietary Nano-Based Filtration – MicronGuardTM:  
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Step 2: QuantumGuardTM & QuantumCoreTM:

[image: ]
[image: ]

[image: ][image: ]
[image: ]

[image: ]


For waste-water systems and reducing waste-water fines and fees.
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MicronGuard™ Breakthrough Technology

* Exceeds nanofiltration results at low pressure:

* 99.9999999% bacteria removal (>9 LRV*)

* 3 party testing conducted at two different laboratories™

* 1.36 psi over 3-filter whole house system

* 99% reduction of heavy metals (includes 97.2% lead reduction)
* 95% reduction of PFAS (forever chemicals, PFOA/PFOS)

* No water loss (no back flushing or wastewater generated), unlike RO
systems

* Does not need to be plumbed to septic or municipal wastewater outlet

* Extremely low pressure drop versus 30-40 psi drop with other whole
house systems

* 10x dirt holding capacity than mechanical filters (spiral wound,
polypropylene, etc.)

* Affordable, low maintenance, installs easily, all parts included, no
electrical or waste connections
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Proprietary Nano-Based Filtration: Targeting unique pathogens/enabling slow release

Proprietary Modifications made to the filtration Enables Technology. This is only possible due to the high capacity
and low pressure attributes of the high surface area pleated substrate.

© QuantumGuard™ - allows surface modification of each filter via mechanical filtration to be able to addqrke
contaminants.

© QuantumCore™ - allows unique resins/sorbents to be placed in the return core of each filtertotargetunusual

toxins using the same filter array. Also allows the release of disinfectants, softening resins, pH adjustment resins,
nutrients, etc.

QuantumGuard
Pak

Technology lowers costs and improves performance.
-

QuantumCore QuantumCore
Conditioning Resin

QuantumCore
Alkalinity




image8.png
Proven by Data: Independent Testing and Early Pilot Results

Third-party testing and real-world trials confirm Toppen’s superior purification and wellness performance. It's not just us,
we've proven or products using approved certified laboratories and protocols.

Independent Lab Testing

Verified 6 - 7 log microbial reduction (>99.9999 % elimination of bacteria and viruses).
PFAS, PFOA, PFOS removal certified to NSF 53 standards.

Achieved zero wastewater output under continuous-flow conditions.

* Maintains constant line pressure during extended use.

Pilot Program Results

» Dental practices (Phase 1 pilots): consistent high-pressure delivery, improved taste, and clinician approval.
* Residential installations: zero maintenance issues, positive consumer feedback on water quality and taste.
» Data under review for NSF/ANSI 42 & 53, hydrogen-water testing, and extended-use durability.

Next Validation Milestones

¢ Clinical collaboration with wellness and dental partners — H, impact on hydration and oxidative
stress.

 Third-party certification expansion: NSF/ANSI 58 & 401 P238 (emerging contaminants).

¢ Lifecycle testing for cartridge longevity and mineral delivery stability.
ientific validation underpins Toppen’s differentiation - proven purity, functional enhancement, and sustainable performance ready
for scale.
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Toppen'’s Filteration Vs Traditional Water Filteration

Removes Toppen Reverse Osmo:

PFAS (forever chemicals)

Bacteriq, spores, cysts

Heavy metals (like arsenic, lead, and mercury)

Pesticides, trace pharmaceuticals

Microplastics and other particulates

Features Toppen Reverse Osmosis
- ° ®
° ®
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High flow rate

S

No waste water
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Zero-Waste Filtration: Environmental Innovation at Its Core
Our CleanWater Systems reduce plastic waste, conserve water while applying the top-efficiency design.

How Important is Plastic Waste Reduction?
Example:Annual amount of water bottles for a family of three household...

Sustainability

Each water bottle filter is viable for 500
gallons That is equivalent to 2,000 water
bottles. After consuming 500 gallons of water,
another bottle is not required, only a
replacement filter.

Bottled Water Quality:
-Usually devoid of minerals
-High in micro plastics
-Does not have to meet Safe Water
Drinking Act standards as bottled water is
classified under food regulations

Our Water Bottle Quality:
-PFAS/PFOA/PFOS removed
-Chlorine removed
-Micro plastics removed
-Pesticides removed
-Pharmaceutical removed
-Lead removed
-Bacteria, virus, cysts and spores removed

motte Esimated cost @29 5ot . f
SEliaion @ %0 S e @29 ssbotie NSF certified

84 Cases
2,016 Bottles

Vitapure’s technology inherently supports sustainability by delivering cleaner water with less waste, less plastic, and less energy use.

EEE———
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QuantumRegen
New method to reactivate activated carbon filters in-situ

 Reactivates any form of activated carbon to over 99% of original performance specifications.

* Regeneration is accomplished in-situ/in any vessel containing carbon product.

* Process takes one to two hours.

 In PFAS applications, does not generate a hazardous waste as organic molecules are oxidized.
* Powdered product applied via dissolvable packs that are placed in vessels. (Ease of application)

PurBright
Pool/Spa technology that generates a stabilized hydrogen peroxide and saturated oxygen

* Produces high clarity water.

* Stabilizes water pH and alkalinity.

* Non-damaging to skin.

 Dissolved oxygen provides health benefits
* No chlorine or other nasty odors.
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Closing the Loop: Regenerative Water Treatment Opportun
Regenerative Carbon Technology for Sustainable Wastewater Treatment

S

Vitapure applies advanced, in-situ carbon regeneration processes to capture, restore, and reuse carbon filtration media—delivering high-
performance contaminant removal without the waste, chemicals, hauling costs or inefficiencies and liabilities of traditional systems.

KEY DIFFERENTIATORS Contaminated

¢ Closed-Loop System — Minimizes or eliminates carbon disposal and transportation costs ’ Water ‘

* Reduced Operating Costs — Less media replacement and handling

« In-situ regeneration eliminates RCRA liability in hazardous waste hauling CarbonFiltiation Garbion Filration
* Lower Environmental Impact — No landfill waste, reduced chemical usage

* High Contaminant Removal — Effective on emerging contaminants (PFAS, pharmaceuticals, C‘

micro plastics)

 Scalable Design — Applicable across industrial, municipal, and commercial systems ‘ ‘

Regeneration _ Reuse
MARKET CONTEXT

Industrial / Commercial Opportunity: $20B+ global market 6-7% CAGR growth HOW IT WORKS
Driven by: Capture: High-surface-area carbon adsorbs contaminants including
* Sustainability mandates PFAS, VOCs, metals, and organics
« PFAS / emerging contaminant regulations Regenerate: Carbon is restored through proprietary regenerative
« Infrastructure modernization advanced oxidation process) that is done on - site.
* Water reuse initiatives Reuse: Media is returned to service—eliminating constant replacement

and waste streams
Repeat: Continuous cycle reduces operating cost and environmental
impact

From Zero Waste to Wastewater Solutions—Vitapure delivers a complete, sustainable
water lifecycle strategy.
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Proprietary Nano-Based Filtration: Engineered for Absolute Purity, health benefits and cost reduction.
Our patented filters deliver extreme purification without pressure loss or wastewater.

© Multi-stage nano-filtration removes >99.99999% of bacteria and >99.9999% of viruses.

© Certified to NSF 42 for Particulate Class I, MicroPlastics, bacteria, spores, cysts, parasites, pathogens.
© Certified to NSF 53 for PFAS, PFOA, and PFOS removal.

© Removes heavy metals, pesticides, microplastics, and pharmaceuticals.

© Zero-wastewater — unlike reverse osmosis (RO) systems that discard 50-80 % of input water and reduce flow
pressure.

© Scalable design — from under-sink units to high-volume industrial applications.

Constant Pressure Flow — No pumps, no tanks, no performance loss. It's simple.

6

barrier Nano-active capture Pol yer

Outer layer / prefiltration capturing Proprietary mixes... membrane-like Post-treatment... improves taste, balance,
particulates and cysts elements targeting toxins and performance consistency
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Alkaline Enrichment: Water That Supports Wellness
Adds beneficial minerals to promote balance, hydration, and vitality. Simply applied to existing systems.

Toppen’s nano-engineered filters deliver extreme purification without pressure loss or wastewater.
© Mineral-release layer reintroduces calcium, magnesium, and trace elements - restoring natural balance and better
taste.

© Mineral impact on molecular H,, neutralizes oxidative stress and enhances cellular hydration.
© Optimized pH (8-9) creates alkaline balance without over-mineralizing. Feels SMOOTH.

© Combined filtration + enhancements deliver safety and functional benefit efficiently - small system footprint.

© Designed for consistent mineral delivery and no pressure loss during enrichment.

° e e Purified Water

Mineral catalyst
Mineral re-balance, pH optimization

e Hydrogen-Alkaline Water

=

nano-membrane Polish layer
active capture

Mechanical barrier
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Proprietary Nano-Based Filtration: Targeting unique pathogens/enabling slow release

Proprietary Modifications made to the filtration Enables Technology. This is only possible due to the high capacity
and low pressure attributes of the high surface area pleated substrate.

© QuantumGuard™ - allows surface modification of each filter via mechanical filtration to be able to addqrke
contaminants.

© QuantumCore™ - allows unique resins/sorbents to be placed in the return core of each filtertotargetunusual

toxins using the same filter array. Also allows the release of disinfectants, softening resins, pH adjustment resins,
nutrients, etc.

QuantumGuard
Pak

Technology lowers costs and improves performance.
-

QuantumCore QuantumCore
Conditioning Resin

QuantumCore
Alkalinity
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Zero-Waste Filtration: Environmental Innovation at Its Core
Toppen's innovative technology reduces plastic waste, conserving water through responsible, high-efficiency design.

PURIFY

Zero-Wastewater Performance

- Uses 100% of input water with no
wastewater discharge.

- Avoids the 50-80% water loss seen in typical
RO systems.

- Supports responsible water use in homes,
clinics, and industry.

ENHANCE

Plastic Waste Reduction

© Replaces bottled-water use in residential
and hydration markets.

© Each installed system can eliminate 1,000~
1,500 plastic bottles per month for a family
of four.

© Lower plastic disposal, fewer microplastics,
cleaner water.

&

SUSTAIN

Lower Carbon Impact

© Eliminates emissions from bottled water
manufacturing and transport.

© Reduces ~150-250 kg CO, per household
per year.

© Long-life filters and recyclable components
reduce long-term footprint.

Toppen’s technology inherently supports sustainability. Delivering cleaner water with less waste, less plastic, less energy - at the lowest price possible.
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Passed NSF
Standard 42

(Classl Particulate, Cysts, Extraction
Testing)

Passed NSF
Standard 53

(PFOA/PFOS) less than 20 Parts Per Trillion
(10PPT PFOA/10PPT PFOS) Chlorine
Reduction, Extraction Testing Selection
colors

Passed NSF
Standard 61

(Extraction Testing, Pressure Testing)




