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The UltraSafe SS System filters use a proprietary patented electro-positive filter media that rapidly adsorbs particles, as small as a few nanometers. 
· Advanced Ultra Filtration
· Great tasting water
· NSF certified, 42, 53, 61, 372
· No Chemicals
· Large capacity filters
· Annual change out in most applications
· Water softening (Optional on request)
· Low cost to maintain
· Easy to maintain
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SKU T-50202-01 Shop | Ultra Home 
UltraSafe SS System – Well Water
UltraSafe SS System™
Filtration System for Under 10 - 20 GPM

Quality Water For Your Whole House.
The UltraHome Filtration System is your clean water solution for you & your family. It creates healthy water for drinking, cleaning, and bathing. Our filtration system uses the same technology used by NASA. It filters water with no chemicals. The UltraHome Filtration System creates healthy and great tasting water for your family to enjoy.

Purer Then Bottle Water

Saving the planet, replacing bottled water with UltraHome Filtration System.
· No Chemicals.
· 99.999999% Removal of Bacteria
· >99.99% Removal of Spores, Bacteria, Cysts
· PFAS / PFOS / PFOA – Forever Chemicals
· Viruses, pathogens, mold, fungus
· ‘Allowable Toxins’ – chlorine
· Heavy Metals, Lead, Micro-Plastics
· Pesticides, Pharmaceuticals
· Adding Micro-Nutrients & Minerals for Optimum Health benefits
· Eco-Friendly
· Eliminates the use for plastic water bottles
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Unit Price:		$2,099.00
Tax (Varies)		$
Shipping  (Varies)	$
Total			$
Button - Proceed to Check-Out…CC Authorization, etc.
Input mailing address, cc info, billing, emailSplit Order to Toppen, Funds, Order, Order #, Subtotal, Transfer of funds including shipping, Toppen packages and ships, needs packing slip.
Never question what is in your water again.



image4.png
CleanWaterCleanAir.com
email: Morelnfo.CWCA@gmail.com
www.CleanWaterCleanAir.com





image30.png
CleanWaterCleanAir.com
email: Morelnfo.CWCA@gmail.com
www.CleanWaterCleanAir.com





image1.png




image2.png
Passed NSF
Standard 42

(Classl Particulate, Cysts, Extraction
Testing)

Passed NSF
Standard 53

(PFOA/PFOS) less than 20 Parts Per Trillion
(10PPT PFOA/10PPT PFOS) Chlorine
Reduction, Extraction Testing Selection
colors

Passed NSF
Standard 61

(Extraction Testing, Pressure Testing)
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